(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A3")
	(layers
		(0 "F.Cu" signal "TOP")
		(4 "In1.Cu" signal "L2_GND")
		(6 "In2.Cu" signal "L3_SIG")
		(8 "In3.Cu" signal "L4_GND")
		(10 "In4.Cu" signal "L5_VCC")
		(12 "In5.Cu" signal "L6_SIG")
		(14 "In6.Cu" signal "L7_GND")
		(2 "B.Cu" signal "BOTTOM")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user "Package Geometry/Pastemask Top")
		(15 "B.Paste" user "Package Geometry/Pastemask Bottom")
		(5 "F.SilkS" user "Ref Des/Silkscreen Top")
		(7 "B.SilkS" user "Ref Des/Silkscreen Bottom")
		(1 "F.Mask" user "Board Geometry/Soldermask Top")
		(3 "B.Mask" user "Board Geometry/Soldermask Bottom")
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user "Board Geometry/Outline")
		(27 "Margin" user)
		(31 "F.CrtYd" user "Package Geometry/Place Bound Top")
		(29 "B.CrtYd" user "Package Geometry/Place Bound Bottom")
		(35 "F.Fab" user "Ref Des/Assembly Top")
		(33 "B.Fab" user "Ref Des/Assembly Bottom")
		(39 "User.1" user "DIMENSION")
		(41 "User.2" user "BOT-DXF-L")
		(43 "User.3" user "PASTEMASK_TOP")
		(45 "User.4" user "PASTEMASK_BOTTOM")
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
		(57 "User.10" user)
		(59 "User.11" user)
		(61 "User.12" user)
		(63 "User.13" user)
		(65 "User.14" user)
		(67 "User.15" user)
		(69 "User.16" user)
		(71 "User.17" user)
		(73 "User.18" user)
		(75 "User.19" user)
		(77 "User.20" user)
		(79 "User.21" user)
		(81 "User.22" user)
		(83 "User.23" user)
		(85 "User.24" user)
		(87 "User.25" user)
		(89 "User.26" user)
		(91 "User.27" user)
		(93 "User.28" user)
		(95 "User.29" user)
		(97 "User.30" user)
		(99 "User.31" user)
		(101 "User.32" user)
		(103 "User.33" user)
		(105 "User.34" user)
		(107 "User.35" user)
		(109 "User.36" user)
		(111 "User.37" user)
		(113 "User.38" user)
		(115 "User.39" user)
		(117 "User.40" user)
		(119 "User.41" user)
		(121 "User.42" user)
		(123 "User.43" user)
		(125 "User.44" user)
		(127 "User.45" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 312.049942 173.649984)
		(property "Reference" "J29"
			(at -0.489204 3.886708 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Reference" "${REFERENCE}"
			(at 0 -0.28575 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "19.69"
			(at -17.272 4.34975 0)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "0.5"
			(at -13.3096 4.34975 0)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "1220.48"
			(at -2.3114 -5.93725 0)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "31"
			(at 2.7686 -5.93725 0)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "157.48"
			(at 16.5354 0.15875 0)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "4"
			(at 21.0566 0.15875 0)
			(unlocked yes)
			(layer "User.1")
		)
		(pad "" np_thru_hole circle
			(at -16.050006 -1.199896)
			(size 0.8001 0.8001)
			(drill 0.8001)
			(layers "*.Cu" "*.Mask")
			(clearance 0.178816)
		)
		(pad "" np_thru_hole circle
			(at 16.050006 -1.199896)
			(size 0.8001 0.8001)
			(drill 0.8001)
			(layers "*.Cu" "*.Mask")
			(clearance 0.178816)
		)
		(pad "1" smd rect
			(at -14.74978 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "2" smd rect
			(at -14.74978 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "3" smd rect
			(at -14.249908 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "4" smd rect
			(at -14.249908 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "5" smd rect
			(at -13.750036 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "6" smd rect
			(at -13.750036 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "7" smd rect
			(at -13.24991 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "8" smd rect
			(at -13.24991 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "9" smd rect
			(at -12.750038 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "10" smd rect
			(at -12.750038 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "11" smd rect
			(at -12.249912 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "12" smd rect
			(at -12.249912 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+12V")
		)
		(pad "13" smd rect
			(at -11.75004 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "14" smd rect
			(at -11.75004 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "15" smd rect
			(at -11.249914 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_RX_HPD")
		)
		(pad "16" smd rect
			(at -11.249914 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX0_HPD")
		)
		(pad "17" smd rect
			(at -10.750042 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_RX_DSDA")
		)
		(pad "18" smd rect
			(at -10.750042 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX0_DDC_SDA")
		)
		(pad "19" smd rect
			(at -10.249916 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "20" smd rect
			(at -10.249916 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "21" smd rect
			(at -9.750044 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_RX_DSCL")
		)
		(pad "22" smd rect
			(at -9.750044 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX0_DDC_SCL")
		)
		(pad "23" smd rect
			(at -9.249918 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_RX_PWR_DET")
		)
		(pad "24" smd rect
			(at -9.249918 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX0_OUT_OE")
		)
		(pad "25" smd rect
			(at -8.750046 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_SDA_CTL")
		)
		(pad "26" smd rect
			(at -8.750046 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP_TX_DIS")
		)
		(pad "27" smd rect
			(at -8.24992 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_SCL_CTL")
		)
		(pad "28" smd rect
			(at -8.24992 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PL_485_RXD1")
		)
		(pad "29" smd rect
			(at -7.750048 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "30" smd rect
			(at -7.750048 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "31" smd rect
			(at -7.249922 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP2_LOSS")
		)
		(pad "32" smd rect
			(at -7.249922 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PL_485_DE1")
		)
		(pad "33" smd rect
			(at -6.75005 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP1_LOSS")
		)
		(pad "34" smd rect
			(at -6.75005 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PL_485_TXD1")
		)
		(pad "35" smd rect
			(at -6.249924 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FAN_PWM")
		)
		(pad "36" smd rect
			(at -6.249924 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PL_485_RXD2")
		)
		(pad "37" smd rect
			(at -5.750052 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "8T49N241_RST")
		)
		(pad "38" smd rect
			(at -5.750052 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PL_485_DE2")
		)
		(pad "39" smd rect
			(at -5.249926 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "40" smd rect
			(at -5.249926 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "41" smd rect
			(at -4.750054 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "8T49N241_INT_ALM")
		)
		(pad "42" smd rect
			(at -4.750054 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PL_485_TXD2")
		)
		(pad "43" smd rect
			(at -4.249928 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "8T49N241_LOL")
		)
		(pad "44" smd rect
			(at -4.249928 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_PRSNT")
		)
		(pad "45" smd rect
			(at -3.750056 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "CLK_REC_SCL")
		)
		(pad "46" smd rect
			(at -3.750056 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L10_N")
		)
		(pad "47" smd rect
			(at -3.24993 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "CLK_REC_SDA")
		)
		(pad "48" smd rect
			(at -3.24993 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L10_P")
		)
		(pad "49" smd rect
			(at -2.750058 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "50" smd rect
			(at -2.750058 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "51" smd rect
			(at -2.249932 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "CAM_SDA")
		)
		(pad "52" smd rect
			(at -2.249932 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L3_N")
		)
		(pad "53" smd rect
			(at -1.75006 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "CAM_SCL")
		)
		(pad "54" smd rect
			(at -1.75006 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L3_P")
		)
		(pad "55" smd rect
			(at -1.249934 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "CAM_GPIO")
		)
		(pad "56" smd rect
			(at -1.249934 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L12_N")
		)
		(pad "57" smd rect
			(at -0.750062 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "CAM_CLK")
		)
		(pad "58" smd rect
			(at -0.750062 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L12_P")
		)
		(pad "59" smd rect
			(at -0.249936 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "60" smd rect
			(at -0.249936 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "61" smd rect
			(at 0.249936 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PL_KEY")
		)
		(pad "62" smd rect
			(at 0.249936 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L7_N")
		)
		(pad "63" smd rect
			(at 0.750062 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PL_LED")
		)
		(pad "64" smd rect
			(at 0.750062 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L7_P")
		)
		(pad "65" smd rect
			(at 1.249934 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PL_UART_RX")
		)
		(pad "66" smd rect
			(at 1.249934 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L6_N")
		)
		(pad "67" smd rect
			(at 1.75006 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PL_UART_TX")
		)
		(pad "68" smd rect
			(at 1.75006 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PWRGD")
		)
		(pad "69" smd rect
			(at 2.249932 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "70" smd rect
			(at 2.249932 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "71" smd rect
			(at 2.750058 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L4_N")
		)
		(pad "72" smd rect
			(at 2.750058 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA16_N")
		)
		(pad "73" smd rect
			(at 3.24993 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B87_L4_P")
		)
		(pad "74" smd rect
			(at 3.24993 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA16_P")
		)
		(pad "75" smd rect
			(at 3.750056 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA15_N")
		)
		(pad "76" smd rect
			(at 3.750056 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA14_N")
		)
		(pad "77" smd rect
			(at 4.249928 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA15_P")
		)
		(pad "78" smd rect
			(at 4.249928 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA14_P")
		)
		(pad "79" smd rect
			(at 4.750054 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "80" smd rect
			(at 4.750054 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "81" smd rect
			(at 5.249926 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA11_N")
		)
		(pad "82" smd rect
			(at 5.249926 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA13_N")
		)
		(pad "83" smd rect
			(at 5.750052 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA11_P")
		)
		(pad "84" smd rect
			(at 5.750052 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA13_P")
		)
		(pad "85" smd rect
			(at 6.249924 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA12_N")
		)
		(pad "86" smd rect
			(at 6.249924 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA10_N")
		)
		(pad "87" smd rect
			(at 6.75005 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA12_P")
		)
		(pad "88" smd rect
			(at 6.75005 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA10_P")
		)
		(pad "89" smd rect
			(at 7.249922 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "90" smd rect
			(at 7.249922 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "91" smd rect
			(at 7.750048 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA09_N")
		)
		(pad "92" smd rect
			(at 7.750048 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA08_N")
		)
		(pad "93" smd rect
			(at 8.24992 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA09_P")
		)
		(pad "94" smd rect
			(at 8.24992 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA08_P")
		)
		(pad "95" smd rect
			(at 8.750046 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA07_N")
		)
		(pad "96" smd rect
			(at 8.750046 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA06_N")
		)
		(pad "97" smd rect
			(at 9.249918 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA07_P")
		)
		(pad "98" smd rect
			(at 9.249918 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA06_P")
		)
		(pad "99" smd rect
			(at 9.750044 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "100" smd rect
			(at 9.750044 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "101" smd rect
			(at 10.249916 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_UART_TX")
		)
		(pad "102" smd rect
			(at 10.249916 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_68")
		)
		(pad "103" smd rect
			(at 10.750042 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_MIO26")
		)
		(pad "104" smd rect
			(at 10.750042 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_RESET_N")
		)
		(pad "105" smd rect
			(at 11.249914 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "DP_AUX_OUT_MIO27")
		)
		(pad "106" smd rect
			(at 11.249914 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_IIC0_SDA")
		)
		(pad "107" smd rect
			(at 11.75004 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_MIO31")
		)
		(pad "108" smd rect
			(at 11.75004 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_MIO36")
		)
		(pad "109" smd rect
			(at 12.249912 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_CAN2_TX")
		)
		(pad "110" smd rect
			(at 12.249912 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RSTN_MIO37")
		)
		(pad "111" smd rect
			(at 12.750038 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_LED")
		)
		(pad "112" smd rect
			(at 12.750038 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "DP_OE_MIO29")
		)
		(pad "113" smd rect
			(at 13.24991 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_CAN1_TX")
		)
		(pad "114" smd rect
			(at 13.24991 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "DP_AUX_IN_MIO30")
		)
		(pad "115" smd rect
			(at 13.750036 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_KEY")
		)
		(pad "116" smd rect
			(at 13.750036 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_IIC0_SCL")
		)
		(pad "117" smd rect
			(at 14.249908 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_CAN2_RX")
		)
		(pad "118" smd rect
			(at 14.249908 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_UART_RX")
		)
		(pad "119" smd rect
			(at 14.74978 1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "DP_HPD_MIO28")
		)
		(pad "120" smd rect
			(at 14.74978 -1.649984)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_CAN1_RX")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 313.076102 199.887676 180)
		(property "Reference" ""
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Reference" "${REFERENCE}"
			(at -2.6416 1.64465 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "50"
			(at 47.7012 -0.52705 180)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "1968.50"
			(at 42.672 -0.52705 180)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "70"
			(at 0.7874 -33.01365 180)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "2755.91"
			(at -4.2418 -33.01365 180)
			(unlocked yes)
			(layer "User.1")
		)
		(pad "" np_thru_hole circle
			(at -34.99993 -24.99995 180)
			(size 6.35 6.35)
			(drill 2.999994)
			(layers "*.Cu" "*.Mask")
			(clearance 0.3175)
			(padstack
				(mode front_inner_back)
				(layer "Inner"
					(shape circle)
					(size 2.999994 2.999994)
					(clearance 1.992376)
				)
				(layer "B.Cu"
					(shape circle)
					(size 6.35 6.35)
					(clearance 0.3175)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -34.99993 24.99995 180)
			(size 6.35 6.35)
			(drill 2.999994)
			(layers "*.Cu" "*.Mask")
			(clearance 0.3175)
			(padstack
				(mode front_inner_back)
				(layer "Inner"
					(shape circle)
					(size 2.999994 2.999994)
					(clearance 1.992376)
				)
				(layer "B.Cu"
					(shape circle)
					(size 6.35 6.35)
					(clearance 0.3175)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 34.99993 -24.99995 180)
			(size 6.35 6.35)
			(drill 2.999994)
			(layers "*.Cu" "*.Mask")
			(clearance 0.3175)
			(padstack
				(mode front_inner_back)
				(layer "Inner"
					(shape circle)
					(size 2.999994 2.999994)
					(clearance 1.992376)
				)
				(layer "B.Cu"
					(shape circle)
					(size 6.35 6.35)
					(clearance 0.3175)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 34.99993 24.99995 180)
			(size 6.35 6.35)
			(drill 2.999994)
			(layers "*.Cu" "*.Mask")
			(clearance 0.3175)
			(padstack
				(mode front_inner_back)
				(layer "Inner"
					(shape circle)
					(size 2.999994 2.999994)
					(clearance 1.992376)
				)
				(layer "B.Cu"
					(shape circle)
					(size 6.35 6.35)
					(clearance 0.3175)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 276.815316 199.869642 90)
		(property "Reference" "J32"
			(at -7.999984 3.965956 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Reference" "${REFERENCE}"
			(at 0 -0.28575 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "31"
			(at 2.7686 -5.93725 90)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "1220.48"
			(at -2.3114 -5.93725 90)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "4"
			(at 21.0566 0.15875 90)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "157.48"
			(at 16.5354 0.15875 90)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "0.5"
			(at -13.3096 4.34975 90)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "19.69"
			(at -17.272 4.34975 90)
			(unlocked yes)
			(layer "User.1")
		)
		(pad "" np_thru_hole circle
			(at -16.050006 -1.199896 90)
			(size 0.8001 0.8001)
			(drill 0.8001)
			(layers "*.Cu" "*.Mask")
			(clearance 0.178816)
		)
		(pad "" np_thru_hole circle
			(at 16.050006 -1.199896 90)
			(size 0.8001 0.8001)
			(drill 0.8001)
			(layers "*.Cu" "*.Mask")
			(clearance 0.178816)
		)
		(pad "1" smd rect
			(at -14.74978 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX0_P")
		)
		(pad "2" smd rect
			(at -14.74978 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX0_P")
		)
		(pad "3" smd rect
			(at -14.249908 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX0_N")
		)
		(pad "4" smd rect
			(at -14.249908 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX0_N")
		)
		(pad "5" smd rect
			(at -13.750036 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "6" smd rect
			(at -13.750036 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "7" smd rect
			(at -13.24991 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX1_P")
		)
		(pad "8" smd rect
			(at -13.24991 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX1_P")
		)
		(pad "9" smd rect
			(at -12.750038 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX1_N")
		)
		(pad "10" smd rect
			(at -12.750038 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX1_N")
		)
		(pad "11" smd rect
			(at -12.249912 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "12" smd rect
			(at -12.249912 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "13" smd rect
			(at -11.75004 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX2_P")
		)
		(pad "14" smd rect
			(at -11.75004 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX2_P")
		)
		(pad "15" smd rect
			(at -11.249914 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX2_N")
		)
		(pad "16" smd rect
			(at -11.249914 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX2_N")
		)
		(pad "17" smd rect
			(at -10.750042 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "18" smd rect
			(at -10.750042 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "19" smd rect
			(at -10.249916 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX3_P")
		)
		(pad "20" smd rect
			(at -10.249916 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX3_P")
		)
		(pad "21" smd rect
			(at -9.750044 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX3_N")
		)
		(pad "22" smd rect
			(at -9.750044 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX3_N")
		)
		(pad "23" smd rect
			(at -9.249918 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "24" smd rect
			(at -9.249918 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "25" smd rect
			(at -8.750046 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "223_CLK1_P")
		)
		(pad "26" smd rect
			(at -8.750046 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_CLK_P")
		)
		(pad "27" smd rect
			(at -8.24992 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "223_CLK1_N")
		)
		(pad "28" smd rect
			(at -8.24992 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_CLK_N")
		)
		(pad "29" smd rect
			(at -7.750048 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "30" smd rect
			(at -7.750048 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "31" smd rect
			(at -7.249922 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX4_P")
		)
		(pad "32" smd rect
			(at -7.249922 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX4_P")
		)
		(pad "33" smd rect
			(at -6.75005 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX4_N")
		)
		(pad "34" smd rect
			(at -6.75005 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX4_N")
		)
		(pad "35" smd rect
			(at -6.249924 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "36" smd rect
			(at -6.249924 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "37" smd rect
			(at -5.750052 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX5_P")
		)
		(pad "38" smd rect
			(at -5.750052 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX5_P")
		)
		(pad "39" smd rect
			(at -5.249926 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX5_N")
		)
		(pad "40" smd rect
			(at -5.249926 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX5_N")
		)
		(pad "41" smd rect
			(at -4.750054 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "42" smd rect
			(at -4.750054 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "43" smd rect
			(at -4.249928 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX6_P")
		)
		(pad "44" smd rect
			(at -4.249928 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX6_P")
		)
		(pad "45" smd rect
			(at -3.750056 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX6_N")
		)
		(pad "46" smd rect
			(at -3.750056 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX6_N")
		)
		(pad "47" smd rect
			(at -3.24993 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "48" smd rect
			(at -3.24993 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "49" smd rect
			(at -2.750058 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX7_P")
		)
		(pad "50" smd rect
			(at -2.750058 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX7_P")
		)
		(pad "51" smd rect
			(at -2.249932 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX7_N")
		)
		(pad "52" smd rect
			(at -2.249932 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX7_N")
		)
		(pad "53" smd rect
			(at -1.75006 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "54" smd rect
			(at -1.75006 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "55" smd rect
			(at -1.249934 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "224_CLK1_P")
		)
		(pad "56" smd rect
			(at -1.249934 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "224_CLK0_P")
		)
		(pad "57" smd rect
			(at -0.750062 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "224_CLK1_N")
		)
		(pad "58" smd rect
			(at -0.750062 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "224_CLK0_N")
		)
		(pad "59" smd rect
			(at -0.249936 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "60" smd rect
			(at -0.249936 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "61" smd rect
			(at 0.249936 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_DRU_CLOCK_P")
		)
		(pad "62" smd rect
			(at 0.249936 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "225_SFP_CLKP")
		)
		(pad "63" smd rect
			(at 0.750062 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_DRU_CLOCK_N")
		)
		(pad "64" smd rect
			(at 0.750062 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "225_SFP_CLKN")
		)
		(pad "65" smd rect
			(at 1.249934 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "66" smd rect
			(at 1.249934 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "67" smd rect
			(at 1.75006 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_DP0_M2C_P")
		)
		(pad "68" smd rect
			(at 1.75006 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP1_RX_P")
		)
		(pad "69" smd rect
			(at 2.249932 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_DP0_M2C_N")
		)
		(pad "70" smd rect
			(at 2.249932 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP1_RX_N")
		)
		(pad "71" smd rect
			(at 2.750058 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "72" smd rect
			(at 2.750058 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "73" smd rect
			(at 3.24993 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_DP0_C2M_P")
		)
		(pad "74" smd rect
			(at 3.24993 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP1_TX_P")
		)
		(pad "75" smd rect
			(at 3.750056 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_DP0_C2M_N")
		)
		(pad "76" smd rect
			(at 3.750056 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP1_TX_N")
		)
		(pad "77" smd rect
			(at 4.249928 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "78" smd rect
			(at 4.249928 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "79" smd rect
			(at 4.750054 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "225_RX2_P")
		)
		(pad "80" smd rect
			(at 4.750054 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP2_RX_P")
		)
		(pad "81" smd rect
			(at 5.249926 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "225_RX2_N")
		)
		(pad "82" smd rect
			(at 5.249926 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP2_RX_N")
		)
		(pad "83" smd rect
			(at 5.750052 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "84" smd rect
			(at 5.750052 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "85" smd rect
			(at 6.249924 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "225_TX2_P")
		)
		(pad "86" smd rect
			(at 6.249924 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP2_TX_P")
		)
		(pad "87" smd rect
			(at 6.75005 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "225_TX2_N")
		)
		(pad "88" smd rect
			(at 6.75005 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SFP2_TX_N")
		)
		(pad "89" smd rect
			(at 7.249922 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "90" smd rect
			(at 7.249922 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "91" smd rect
			(at 7.750048 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_IN0_RX_CLKP")
		)
		(pad "92" smd rect
			(at 7.750048 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_8T49N241_OUT_P")
		)
		(pad "93" smd rect
			(at 8.24992 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_IN0_RX_CLKN")
		)
		(pad "94" smd rect
			(at 8.24992 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_8T49N241_OUT_N")
		)
		(pad "95" smd rect
			(at 8.750046 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "96" smd rect
			(at 8.750046 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "97" smd rect
			(at 9.249918 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "226_RX3_P")
		)
		(pad "98" smd rect
			(at 9.249918 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "226_TX3_P")
		)
		(pad "99" smd rect
			(at 9.750044 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "226_RX3_N")
		)
		(pad "100" smd rect
			(at 9.750044 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "226_TX3_N")
		)
		(pad "101" smd rect
			(at 10.249916 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "102" smd rect
			(at 10.249916 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "103" smd rect
			(at 10.750042 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_IN0_RX_2P")
		)
		(pad "104" smd rect
			(at 10.750042 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX0_D2P")
		)
		(pad "105" smd rect
			(at 11.249914 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_IN0_RX_2N")
		)
		(pad "106" smd rect
			(at 11.249914 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX0_D2N")
		)
		(pad "107" smd rect
			(at 11.75004 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "108" smd rect
			(at 11.75004 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "109" smd rect
			(at 12.249912 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_IN0_RX_1P")
		)
		(pad "110" smd rect
			(at 12.249912 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX0_D1P")
		)
		(pad "111" smd rect
			(at 12.750038 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_IN0_RX_1N")
		)
		(pad "112" smd rect
			(at 12.750038 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX0_D1N")
		)
		(pad "113" smd rect
			(at 13.24991 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "114" smd rect
			(at 13.24991 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "115" smd rect
			(at 13.750036 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_IN0_RX_0P")
		)
		(pad "116" smd rect
			(at 13.750036 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX0_D0P")
		)
		(pad "117" smd rect
			(at 14.249908 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_IN0_RX_0N")
		)
		(pad "118" smd rect
			(at 14.249908 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX0_D0N")
		)
		(pad "119" smd rect
			(at 14.74978 1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "120" smd rect
			(at 14.74978 -1.649984 90)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 349.29066 199.869642 -90)
		(property "Reference" "J30"
			(at 2.574036 3.958336 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Reference" "${REFERENCE}"
			(at 0 -0.28575 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "19.69"
			(at -17.272 4.34975 270)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "0.5"
			(at -13.3096 4.34975 270)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "157.48"
			(at 16.5354 0.15875 270)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "4"
			(at 21.0566 0.15875 270)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "1220.48"
			(at -2.3114 -5.93725 270)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "31"
			(at 2.7686 -5.93725 270)
			(unlocked yes)
			(layer "User.1")
		)
		(pad "" np_thru_hole circle
			(at -16.050006 -1.199896 270)
			(size 0.8001 0.8001)
			(drill 0.8001)
			(layers "*.Cu" "*.Mask")
			(clearance 0.178816)
		)
		(pad "" np_thru_hole circle
			(at 16.050006 -1.199896 270)
			(size 0.8001 0.8001)
			(drill 0.8001)
			(layers "*.Cu" "*.Mask")
			(clearance 0.178816)
		)
		(pad "1" smd rect
			(at -14.74978 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA02_P")
		)
		(pad "2" smd rect
			(at -14.74978 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SD_D2")
		)
		(pad "3" smd rect
			(at -14.249908 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA02_N")
		)
		(pad "4" smd rect
			(at -14.249908 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SD_D3")
		)
		(pad "5" smd rect
			(at -13.750036 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "6" smd rect
			(at -13.750036 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "7" smd rect
			(at -13.24991 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_CLK0_N")
		)
		(pad "8" smd rect
			(at -13.24991 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SD_CMD")
		)
		(pad "9" smd rect
			(at -12.750038 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_CLK0_P")
		)
		(pad "10" smd rect
			(at -12.750038 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SD_D0")
		)
		(pad "11" smd rect
			(at -12.249912 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA00_CC_P")
		)
		(pad "12" smd rect
			(at -12.249912 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SD_D1")
		)
		(pad "13" smd rect
			(at -11.75004 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA00_CC_N")
		)
		(pad "14" smd rect
			(at -11.75004 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SD_CLK")
		)
		(pad "15" smd rect
			(at -11.249914 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "16" smd rect
			(at -11.249914 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "17" smd rect
			(at -10.750042 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA03_N")
		)
		(pad "18" smd rect
			(at -10.750042 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SD_CD")
		)
		(pad "19" smd rect
			(at -10.249916 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA03_P")
		)
		(pad "20" smd rect
			(at -10.249916 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_57")
		)
		(pad "21" smd rect
			(at -9.750044 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA04_P")
		)
		(pad "22" smd rect
			(at -9.750044 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_STP")
		)
		(pad "23" smd rect
			(at -9.249918 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA04_N")
		)
		(pad "24" smd rect
			(at -9.249918 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DIR")
		)
		(pad "25" smd rect
			(at -8.750046 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "26" smd rect
			(at -8.750046 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "27" smd rect
			(at -8.24992 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_67")
		)
		(pad "28" smd rect
			(at -8.24992 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_CLK")
		)
		(pad "29" smd rect
			(at -7.750048 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_66")
		)
		(pad "30" smd rect
			(at -7.750048 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_NXT")
		)
		(pad "31" smd rect
			(at -7.249922 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_65")
		)
		(pad "32" smd rect
			(at -7.249922 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DATA0")
		)
		(pad "33" smd rect
			(at -6.75005 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_64")
		)
		(pad "34" smd rect
			(at -6.75005 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DATA1")
		)
		(pad "35" smd rect
			(at -6.249924 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "36" smd rect
			(at -6.249924 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "37" smd rect
			(at -5.750052 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA05_N")
		)
		(pad "38" smd rect
			(at -5.750052 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DATA2")
		)
		(pad "39" smd rect
			(at -5.249926 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA05_P")
		)
		(pad "40" smd rect
			(at -5.249926 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DATA3")
		)
		(pad "41" smd rect
			(at -4.750054 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA01_CC_N")
		)
		(pad "42" smd rect
			(at -4.750054 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DATA4")
		)
		(pad "43" smd rect
			(at -4.249928 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA01_CC_P")
		)
		(pad "44" smd rect
			(at -4.249928 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DATA5")
		)
		(pad "45" smd rect
			(at -3.750056 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "46" smd rect
			(at -3.750056 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "47" smd rect
			(at -3.24993 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_63")
		)
		(pad "48" smd rect
			(at -3.24993 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DATA6")
		)
		(pad "49" smd rect
			(at -2.750058 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_62")
		)
		(pad "50" smd rect
			(at -2.750058 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_DATA7")
		)
		(pad "51" smd rect
			(at -2.249932 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_61")
		)
		(pad "52" smd rect
			(at -2.249932 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_TXD0")
		)
		(pad "53" smd rect
			(at -1.75006 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_60")
		)
		(pad "54" smd rect
			(at -1.75006 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_TXD1")
		)
		(pad "55" smd rect
			(at -1.249934 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "56" smd rect
			(at -1.249934 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "57" smd rect
			(at -0.750062 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_59")
		)
		(pad "58" smd rect
			(at -0.750062 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_TXD2")
		)
		(pad "59" smd rect
			(at -0.249936 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net_58")
		)
		(pad "60" smd rect
			(at -0.249936 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_TXD3")
		)
		(pad "61" smd rect
			(at 0.249936 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_POR_B")
		)
		(pad "62" smd rect
			(at 0.249936 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_TXCK")
		)
		(pad "63" smd rect
			(at 0.750062 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FPGA_DONE")
		)
		(pad "64" smd rect
			(at 0.750062 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_TXCTL")
		)
		(pad "65" smd rect
			(at 1.249934 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "66" smd rect
			(at 1.249934 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "67" smd rect
			(at 1.75006 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_MODE3")
		)
		(pad "68" smd rect
			(at 1.75006 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_RXD3")
		)
		(pad "69" smd rect
			(at 2.249932 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_MODE2")
		)
		(pad "70" smd rect
			(at 2.249932 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_RXD2")
		)
		(pad "71" smd rect
			(at 2.750058 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_MODE1")
		)
		(pad "72" smd rect
			(at 2.750058 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_RXD1")
		)
		(pad "73" smd rect
			(at 3.24993 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PS_MODE0")
		)
		(pad "74" smd rect
			(at 3.24993 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_RXD0")
		)
		(pad "75" smd rect
			(at 3.750056 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "76" smd rect
			(at 3.750056 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "77" smd rect
			(at 4.249928 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "JTAG_TCK")
		)
		(pad "78" smd rect
			(at 4.249928 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_RXCTL")
		)
		(pad "79" smd rect
			(at 4.750054 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "JTAG_TDI")
		)
		(pad "80" smd rect
			(at 4.750054 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_RXCK")
		)
		(pad "81" smd rect
			(at 5.249926 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "JTAG_TMS")
		)
		(pad "82" smd rect
			(at 5.249926 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_MDC")
		)
		(pad "83" smd rect
			(at 5.750052 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FPGA_TDO")
		)
		(pad "84" smd rect
			(at 5.750052 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY1_MDIO")
		)
		(pad "85" smd rect
			(at 6.249924 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "86" smd rect
			(at 6.249924 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "87" smd rect
			(at 6.75005 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_RX3_N")
		)
		(pad "88" smd rect
			(at 6.75005 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GT0_DP_TX_N")
		)
		(pad "89" smd rect
			(at 7.249922 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_RX3_P")
		)
		(pad "90" smd rect
			(at 7.249922 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GT0_DP_TX_P")
		)
		(pad "91" smd rect
			(at 7.750048 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "92" smd rect
			(at 7.750048 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "93" smd rect
			(at 8.24992 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_RX2_N")
		)
		(pad "94" smd rect
			(at 8.24992 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GT1_DP_TX_N")
		)
		(pad "95" smd rect
			(at 8.750046 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_RX2_P")
		)
		(pad "96" smd rect
			(at 8.750046 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GT1_DP_TX_P")
		)
		(pad "97" smd rect
			(at 9.249918 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "98" smd rect
			(at 9.249918 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "99" smd rect
			(at 9.750044 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_SSRXN")
		)
		(pad "100" smd rect
			(at 9.750044 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_SSTXN")
		)
		(pad "101" smd rect
			(at 10.249916 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_SSRXP")
		)
		(pad "102" smd rect
			(at 10.249916 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB_SSTXP")
		)
		(pad "103" smd rect
			(at 10.750042 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "104" smd rect
			(at 10.750042 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "105" smd rect
			(at 11.249914 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX_N")
		)
		(pad "106" smd rect
			(at 11.249914 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX_N")
		)
		(pad "107" smd rect
			(at 11.75004 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RX_P")
		)
		(pad "108" smd rect
			(at 11.75004 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_TX_P")
		)
		(pad "109" smd rect
			(at 12.249912 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "110" smd rect
			(at 12.249912 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "111" smd rect
			(at 12.750038 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_PCIE_REFCLK_N")
		)
		(pad "112" smd rect
			(at 12.750038 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_USB_CLKN")
		)
		(pad "113" smd rect
			(at 13.24991 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_PCIE_REFCLK_P")
		)
		(pad "114" smd rect
			(at 13.24991 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_USB_CLKP")
		)
		(pad "115" smd rect
			(at 13.750036 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "116" smd rect
			(at 13.750036 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "117" smd rect
			(at 14.249908 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_DP_CLKN")
		)
		(pad "118" smd rect
			(at 14.249908 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_CLK3_N")
		)
		(pad "119" smd rect
			(at 14.74978 1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_DP_CLKP")
		)
		(pad "120" smd rect
			(at 14.74978 -1.649984 270)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "505_CLK3_P")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 312.049942 226.125622 180)
		(property "Reference" "J31"
			(at 0.717804 3.931158 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Reference" "${REFERENCE}"
			(at 0 -0.28575 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "4"
			(at 21.0566 0.15875 180)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "157.48"
			(at 16.5354 0.15875 180)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "31"
			(at 2.7686 -5.93725 180)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "1220.48"
			(at -2.3114 -5.93725 180)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "0.5"
			(at -13.3096 4.34975 180)
			(unlocked yes)
			(layer "User.1")
		)
		(fp_text user "19.69"
			(at -17.272 4.34975 180)
			(unlocked yes)
			(layer "User.1")
		)
		(pad "" np_thru_hole circle
			(at -16.050006 -1.199896 180)
			(size 0.8001 0.8001)
			(drill 0.8001)
			(layers "*.Cu" "*.Mask")
			(clearance 0.178816)
		)
		(pad "" np_thru_hole circle
			(at 16.050006 -1.199896 180)
			(size 0.8001 0.8001)
			(drill 0.8001)
			(layers "*.Cu" "*.Mask")
			(clearance 0.178816)
		)
		(pad "1" smd rect
			(at -14.74978 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "POWER_SW")
		)
		(pad "2" smd rect
			(at -14.74978 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VBAT_IN")
		)
		(pad "3" smd rect
			(at -14.249908 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PCIE_RSTN")
		)
		(pad "4" smd rect
			(at -14.249908 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MIPI_LAN0_N")
		)
		(pad "5" smd rect
			(at -13.750036 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_MDIO")
		)
		(pad "6" smd rect
			(at -13.750036 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MIPI_LAN0_P")
		)
		(pad "7" smd rect
			(at -13.24991 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_RESET")
		)
		(pad "8" smd rect
			(at -13.24991 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L18_N")
		)
		(pad "9" smd rect
			(at -12.750038 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_RXCK")
		)
		(pad "10" smd rect
			(at -12.750038 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L18_P")
		)
		(pad "11" smd rect
			(at -12.249912 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "12" smd rect
			(at -12.249912 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "13" smd rect
			(at -11.75004 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_MDC")
		)
		(pad "14" smd rect
			(at -11.75004 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L16_N")
		)
		(pad "15" smd rect
			(at -11.249914 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_RXCTL")
		)
		(pad "16" smd rect
			(at -11.249914 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L16_P")
		)
		(pad "17" smd rect
			(at -10.750042 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_RXD0")
		)
		(pad "18" smd rect
			(at -10.750042 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MIPI_LAN1_N")
		)
		(pad "19" smd rect
			(at -10.249916 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_RXD1")
		)
		(pad "20" smd rect
			(at -10.249916 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MIPI_LAN1_P")
		)
		(pad "21" smd rect
			(at -9.750044 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "22" smd rect
			(at -9.750044 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "23" smd rect
			(at -9.249918 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_RXD2")
		)
		(pad "24" smd rect
			(at -9.249918 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L7_N")
		)
		(pad "25" smd rect
			(at -8.750046 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_RXD3")
		)
		(pad "26" smd rect
			(at -8.750046 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L7_P")
		)
		(pad "27" smd rect
			(at -8.24992 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_TXCTL")
		)
		(pad "28" smd rect
			(at -8.24992 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L21_N")
		)
		(pad "29" smd rect
			(at -7.750048 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_TXD2")
		)
		(pad "30" smd rect
			(at -7.750048 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L21_P")
		)
		(pad "31" smd rect
			(at -7.249922 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "32" smd rect
			(at -7.249922 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "33" smd rect
			(at -6.75005 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_TXD3")
		)
		(pad "34" smd rect
			(at -6.75005 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L6_N")
		)
		(pad "35" smd rect
			(at -6.249924 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_TXCK")
		)
		(pad "36" smd rect
			(at -6.249924 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L6_P")
		)
		(pad "37" smd rect
			(at -5.750052 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_TXD1")
		)
		(pad "38" smd rect
			(at -5.750052 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L17_N")
		)
		(pad "39" smd rect
			(at -5.249926 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "PHY2_TXD0")
		)
		(pad "40" smd rect
			(at -5.249926 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L17_P")
		)
		(pad "41" smd rect
			(at -4.750054 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "42" smd rect
			(at -4.750054 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "43" smd rect
			(at -4.249928 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L15_N")
		)
		(pad "44" smd rect
			(at -4.249928 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L4_N")
		)
		(pad "45" smd rect
			(at -3.750056 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L15_P")
		)
		(pad "46" smd rect
			(at -3.750056 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L4_P")
		)
		(pad "47" smd rect
			(at -3.24993 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L20_N")
		)
		(pad "48" smd rect
			(at -3.24993 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L11_N")
		)
		(pad "49" smd rect
			(at -2.750058 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L20_P")
		)
		(pad "50" smd rect
			(at -2.750058 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L11_P")
		)
		(pad "51" smd rect
			(at -2.249932 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "52" smd rect
			(at -2.249932 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "53" smd rect
			(at -1.75006 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L23_N")
		)
		(pad "54" smd rect
			(at -1.75006 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MIPI_CLK_N")
		)
		(pad "55" smd rect
			(at -1.249934 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L23_P")
		)
		(pad "56" smd rect
			(at -1.249934 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MIPI_CLK_P")
		)
		(pad "57" smd rect
			(at -0.750062 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L22_N")
		)
		(pad "58" smd rect
			(at -0.750062 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L9_N")
		)
		(pad "59" smd rect
			(at -0.249936 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L22_P")
		)
		(pad "60" smd rect
			(at -0.249936 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B65_L9_P")
		)
		(pad "61" smd rect
			(at 0.249936 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "62" smd rect
			(at 0.249936 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "63" smd rect
			(at 0.750062 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_REC_CLOCK_P")
		)
		(pad "64" smd rect
			(at 0.750062 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B64_L9_P")
		)
		(pad "65" smd rect
			(at 1.249934 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_REC_CLOCK_N")
		)
		(pad "66" smd rect
			(at 1.249934 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B64_L9_N")
		)
		(pad "67" smd rect
			(at 1.75006 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B64_L6_P")
		)
		(pad "68" smd rect
			(at 1.75006 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_CLK1_P")
		)
		(pad "69" smd rect
			(at 2.249932 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B64_L6_N")
		)
		(pad "70" smd rect
			(at 2.249932 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_CLK1_N")
		)
		(pad "71" smd rect
			(at 2.750058 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "72" smd rect
			(at 2.750058 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "73" smd rect
			(at 3.24993 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA22_P")
		)
		(pad "74" smd rect
			(at 3.24993 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA17_CC_P")
		)
		(pad "75" smd rect
			(at 3.750056 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA22_N")
		)
		(pad "76" smd rect
			(at 3.750056 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA17_CC_N")
		)
		(pad "77" smd rect
			(at 4.249928 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA21_P")
		)
		(pad "78" smd rect
			(at 4.249928 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA20_P")
		)
		(pad "79" smd rect
			(at 4.750054 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA21_N")
		)
		(pad "80" smd rect
			(at 4.750054 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA20_N")
		)
		(pad "81" smd rect
			(at 5.249926 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "82" smd rect
			(at 5.249926 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "83" smd rect
			(at 5.750052 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA27_P")
		)
		(pad "84" smd rect
			(at 5.750052 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA19_P")
		)
		(pad "85" smd rect
			(at 6.249924 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA27_N")
		)
		(pad "86" smd rect
			(at 6.249924 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA19_N")
		)
		(pad "87" smd rect
			(at 6.75005 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA26_P")
		)
		(pad "88" smd rect
			(at 6.75005 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA23_P")
		)
		(pad "89" smd rect
			(at 7.249922 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA26_N")
		)
		(pad "90" smd rect
			(at 7.249922 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA23_N")
		)
		(pad "91" smd rect
			(at 7.750048 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "92" smd rect
			(at 7.750048 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "93" smd rect
			(at 8.24992 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA25_P")
		)
		(pad "94" smd rect
			(at 8.24992 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA18_CC_P")
		)
		(pad "95" smd rect
			(at 8.750046 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA25_N")
		)
		(pad "96" smd rect
			(at 8.750046 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA18_CC_N")
		)
		(pad "97" smd rect
			(at 9.249918 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B64_L10_P")
		)
		(pad "98" smd rect
			(at 9.249918 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA24_P")
		)
		(pad "99" smd rect
			(at 9.750044 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B64_L10_N")
		)
		(pad "100" smd rect
			(at 9.750044 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA24_N")
		)
		(pad "101" smd rect
			(at 10.249916 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "102" smd rect
			(at 10.249916 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "103" smd rect
			(at 10.750042 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA29_P")
		)
		(pad "104" smd rect
			(at 10.750042 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA31_P")
		)
		(pad "105" smd rect
			(at 11.249914 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA29_N")
		)
		(pad "106" smd rect
			(at 11.249914 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA31_N")
		)
		(pad "107" smd rect
			(at 11.75004 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA28_P")
		)
		(pad "108" smd rect
			(at 11.75004 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA30_P")
		)
		(pad "109" smd rect
			(at 12.249912 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA28_N")
		)
		(pad "110" smd rect
			(at 12.249912 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA30_N")
		)
		(pad "111" smd rect
			(at 12.750038 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "112" smd rect
			(at 12.750038 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
		)
		(pad "113" smd rect
			(at 13.24991 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B64_L22_P")
		)
		(pad "114" smd rect
			(at 13.24991 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA33_P")
		)
		(pad "115" smd rect
			(at 13.750036 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "B64_L22_N")
		)
		(pad "116" smd rect
			(at 13.750036 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA33_N")
		)
		(pad "117" smd rect
			(at 14.249908 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX_LVDS_OUT_P")
		)
		(pad "118" smd rect
			(at 14.249908 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA32_P")
		)
		(pad "119" smd rect
			(at 14.74978 1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "HDMI_TX_LVDS_OUT_N")
		)
		(pad "120" smd rect
			(at 14.74978 -1.649984 180)
			(size 0.249936 2.29997)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "FMC_LA32_N")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 266.676652 162.831108)
		(end 359.926148 162.831108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 266.676652 239.758818)
		(end 266.676652 162.831108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 359.926148 162.831108)
		(end 359.926148 239.758818)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 359.926148 239.758818)
		(end 266.676652 239.758818)
		(layer "Edge.Cuts")
	)
	(gr_text "V2.1"
		(at 355.809316 238.179192 0)
		(layer "B.SilkS")
	)
	(gr_text "FIGURE"
		(at 46.923472 48.668776 0)
		(layer "User.45")
	)
	(gr_text "SIZE"
		(at 82.356472 48.668776 0)
		(layer "User.45")
	)
	(gr_text "8.0"
		(at 82.356472 55.018776 0)
		(layer "User.45")
	)
	(gr_text "19.69"
		(at 82.356472 61.368776 0)
		(layer "User.45")
	)
	(gr_text "27.56"
		(at 82.356472 67.718776 0)
		(layer "User.45")
	)
	(gr_text "27.56"
		(at 82.356472 74.068776 0)
		(layer "User.45")
	)
	(gr_text "35.0"
		(at 82.356472 80.418776 0)
		(layer "User.45")
	)
	(gr_text "36.0"
		(at 82.356472 86.768776 0)
		(layer "User.45")
	)
	(gr_text "40.0"
		(at 82.356472 93.118776 0)
		(layer "User.45")
	)
	(gr_text "42.0"
		(at 82.356472 99.468776 0)
		(layer "User.45")
	)
	(gr_text "43.31"
		(at 82.356472 105.818776 0)
		(layer "User.45")
	)
	(gr_text "51.18"
		(at 82.356472 112.168776 0)
		(layer "User.45")
	)
	(gr_text "62.0"
		(at 82.356472 118.518776 0)
		(layer "User.45")
	)
	(gr_text "70.87"
		(at 82.356472 124.868776 0)
		(layer "User.45")
	)
	(gr_text "90.55"
		(at 82.356472 131.218776 0)
		(layer "User.45")
	)
	(gr_text "106.3"
		(at 82.356472 137.568776 0)
		(layer "User.45")
	)
	(gr_text "118.11"
		(at 82.356472 143.918776 0)
		(layer "User.45")
	)
	(gr_text "118.11"
		(at 82.356472 150.268776 0)
		(layer "User.45")
	)
	(gr_text "125.0"
		(at 82.356472 156.618776 0)
		(layer "User.45")
	)
	(gr_text "31.5"
		(at 82.356472 162.968776 0)
		(layer "User.45")
	)
	(gr_text "43.0"
		(at 82.356472 169.318776 0)
		(layer "User.45")
	)
	(gr_text "50.0"
		(at 82.356472 175.668776 0)
		(layer "User.45")
	)
	(gr_text "53.15"
		(at 82.356472 182.018776 0)
		(layer "User.45")
	)
	(gr_text "63.0"
		(at 82.356472 188.368776 0)
		(layer "User.45")
	)
	(gr_text "129.92"
		(at 82.356472 194.718776 0)
		(layer "User.45")
	)
	(gr_text "55.12x23.62"
		(at 82.356472 201.068776 0)
		(layer "User.45")
	)
	(gr_text "55.12x31.5"
		(at 82.356472 207.418776 0)
		(layer "User.45")
	)
	(gr_text "62.0x39.37"
		(at 82.356472 213.768776 0)
		(layer "User.45")
	)
	(gr_text "74.8x31.5"
		(at 82.356472 220.118776 0)
		(layer "User.45")
	)
	(gr_text "78.74x27.56"
		(at 82.356472 226.468776 0)
		(layer "User.45")
	)
	(gr_text "94.49x31.5"
		(at 82.356472 232.818776 0)
		(layer "User.45")
	)
	(gr_text "102.36x31.5"
		(at 82.356472 239.168776 0)
		(layer "User.45")
	)
	(gr_text "102.36x31.5"
		(at 82.356472 245.518776 0)
		(layer "User.45")
	)
	(gr_text "DRILL CHART: TOP to BOTTOM"
		(at 120.939072 35.968776 0)
		(layer "User.45")
	)
	(gr_text "ALL UNITS ARE IN MILS"
		(at 120.939072 42.318776 0)
		(layer "User.45")
	)
	(gr_text "TOLERANCE"
		(at 130.387872 48.668776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 55.018776 0)
		(layer "User.45")
	)
	(gr_text "+0.0/-0.0"
		(at 130.387872 61.368776 0)
		(layer "User.45")
	)
	(gr_text "+0.0/-0.0"
		(at 130.387872 67.718776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 74.068776 0)
		(layer "User.45")
	)
	(gr_text "+0.0/-0.0"
		(at 130.387872 80.418776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 86.768776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 93.118776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 99.468776 0)
		(layer "User.45")
	)
	(gr_text "+0.0/-0.0"
		(at 130.387872 105.818776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 112.168776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 118.518776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 124.868776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 131.218776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 137.568776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 143.918776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 150.268776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 156.618776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 162.968776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 169.318776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 175.668776 0)
		(layer "User.45")
	)
	(gr_text "+0.0/-0.0"
		(at 130.387872 182.018776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 188.368776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 194.718776 0)
		(layer "User.45")
	)
	(gr_text "+0.0/-0.0"
		(at 130.387872 201.068776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 207.418776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 213.768776 0)
		(layer "User.45")
	)
	(gr_text "+0.0/-0.0"
		(at 130.387872 220.118776 0)
		(layer "User.45")
	)
	(gr_text "+0.0/-0.0"
		(at 130.387872 226.468776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 232.818776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 239.168776 0)
		(layer "User.45")
	)
	(gr_text "+3.0/-3.0"
		(at 130.387872 245.518776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 48.668776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 55.018776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 61.368776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 67.718776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 74.068776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 80.418776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 86.768776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 93.118776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 99.468776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 105.818776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 112.168776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 118.518776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 124.868776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 131.218776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 137.568776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 143.918776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 150.268776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 156.618776 0)
		(layer "User.45")
	)
	(gr_text "NON-PLATED"
		(at 170.545272 162.968776 0)
		(layer "User.45")
	)
	(gr_text "NON-PLATED"
		(at 170.545272 169.318776 0)
		(layer "User.45")
	)
	(gr_text "NON-PLATED"
		(at 170.545272 175.668776 0)
		(layer "User.45")
	)
	(gr_text "NON-PLATED"
		(at 170.545272 182.018776 0)
		(layer "User.45")
	)
	(gr_text "NON-PLATED"
		(at 170.545272 188.368776 0)
		(layer "User.45")
	)
	(gr_text "NON-PLATED"
		(at 170.545272 194.718776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 201.068776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 207.418776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 213.768776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 220.118776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 226.468776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 232.818776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 239.168776 0)
		(layer "User.45")
	)
	(gr_text "PLATED"
		(at 170.545272 245.518776 0)
		(layer "User.45")
	)
	(gr_text "QTY"
		(at 196.529472 48.668776 0)
		(layer "User.45")
	)
	(gr_text "1702"
		(at 196.529472 55.018776 0)
		(layer "User.45")
	)
	(gr_text "10"
		(at 196.529472 61.368776 0)
		(layer "User.45")
	)
	(gr_text "10"
		(at 196.529472 67.718776 0)
		(layer "User.45")
	)
	(gr_text "36"
		(at 196.529472 74.068776 0)
		(layer "User.45")
	)
	(gr_text "10"
		(at 196.529472 80.418776 0)
		(layer "User.45")
	)
	(gr_text "2"
		(at 196.529472 86.768776 0)
		(layer "User.45")
	)
	(gr_text "20"
		(at 196.529472 93.118776 0)
		(layer "User.45")
	)
	(gr_text "12"
		(at 196.529472 99.468776 0)
		(layer "User.45")
	)
	(gr_text "10"
		(at 196.529472 105.818776 0)
		(layer "User.45")
	)
	(gr_text "8"
		(at 196.529472 112.168776 0)
		(layer "User.45")
	)
	(gr_text "2"
		(at 196.529472 118.518776 0)
		(layer "User.45")
	)
	(gr_text "4"
		(at 196.529472 124.868776 0)
		(layer "User.45")
	)
	(gr_text "8"
		(at 196.529472 131.218776 0)
		(layer "User.45")
	)
	(gr_text "2"
		(at 196.529472 137.568776 0)
		(layer "User.45")
	)
	(gr_text "1"
		(at 196.529472 143.918776 0)
		(layer "User.45")
	)
	(gr_text "4"
		(at 196.529472 150.268776 0)
		(layer "User.45")
	)
	(gr_text "4"
		(at 196.529472 156.618776 0)
		(layer "User.45")
	)
	(gr_text "8"
		(at 196.529472 162.968776 0)
		(layer "User.45")
	)
	(gr_text "1"
		(at 196.529472 169.318776 0)
		(layer "User.45")
	)
	(gr_text "2"
		(at 196.529472 175.668776 0)
		(layer "User.45")
	)
	(gr_text "2"
		(at 196.529472 182.018776 0)
		(layer "User.45")
	)
	(gr_text "1"
		(at 196.529472 188.368776 0)
		(layer "User.45")
	)
	(gr_text "4"
		(at 196.529472 194.718776 0)
		(layer "User.45")
	)
	(gr_text "2"
		(at 196.529472 201.068776 0)
		(layer "User.45")
	)
	(gr_text "4"
		(at 196.529472 207.418776 0)
		(layer "User.45")
	)
	(gr_text "2"
		(at 196.529472 213.768776 0)
		(layer "User.45")
	)
	(gr_text "8"
		(at 196.529472 220.118776 0)
		(layer "User.45")
	)
	(gr_text "2"
		(at 196.529472 226.468776 0)
		(layer "User.45")
	)
	(gr_text "4"
		(at 196.529472 232.818776 0)
		(layer "User.45")
	)
	(gr_text "1"
		(at 196.529472 239.168776 0)
		(layer "User.45")
	)
	(gr_text "2"
		(at 196.529472 245.518776 0)
		(layer "User.45")
	)
	(embedded_fonts no)
)
