{
  "board": {
    "3dviewports": [],
    "design_settings": {
      "defaults": {
        "apply_defaults_to_fp_barcodes": false,
        "apply_defaults_to_fp_dimensions": false,
        "apply_defaults_to_fp_fields": false,
        "apply_defaults_to_fp_shapes": false,
        "apply_defaults_to_fp_text": false,
        "board_outline_line_width": 0.05,
        "copper_line_width": 0.2,
        "copper_text_italic": false,
        "copper_text_size_h": 1.5,
        "copper_text_size_v": 1.5,
        "copper_text_thickness": 0.3,
        "copper_text_upright": false,
        "courtyard_line_width": 0.05,
        "dimension_precision": 4,
        "dimension_units": 3,
        "dimensions": {
          "arrow_length": 1270000,
          "extension_offset": 500000,
          "keep_text_aligned": true,
          "suppress_zeroes": true,
          "text_position": 0,
          "units_format": 0
        },
        "fab_line_width": 0.1,
        "fab_text_italic": false,
        "fab_text_size_h": 1.0,
        "fab_text_size_v": 1.0,
        "fab_text_thickness": 0.15,
        "fab_text_upright": false,
        "other_line_width": 0.1,
        "other_text_italic": false,
        "other_text_size_h": 1.0,
        "other_text_size_v": 1.0,
        "other_text_thickness": 0.15,
        "other_text_upright": false,
        "pads": {
          "drill": 0.8,
          "height": 1.27,
          "width": 2.54
        },
        "silk_line_width": 0.1,
        "silk_text_italic": false,
        "silk_text_size_h": 1.0,
        "silk_text_size_v": 1.0,
        "silk_text_thickness": 0.1,
        "silk_text_upright": false,
        "zones": {
          "min_clearance": 0.5
        }
      },
      "diff_pair_dimensions": [],
      "drc_exclusions": [],
      "meta": {
        "filename": "board_design_settings.json",
        "version": 2
      },
      "rule_severities": {
        "annular_width": "error",
        "clearance": "error",
        "connection_width": "warning",
        "copper_edge_clearance": "error",
        "copper_sliver": "warning",
        "courtyards_overlap": "error",
        "creepage": "error",
        "diff_pair_gap_out_of_range": "error",
        "diff_pair_uncoupled_length_too_long": "error",
        "drill_out_of_range": "error",
        "duplicate_footprints": "warning",
        "extra_footprint": "warning",
        "footprint": "error",
        "footprint_filters_mismatch": "ignore",
        "footprint_symbol_field_mismatch": "warning",
        "footprint_symbol_mismatch": "warning",
        "footprint_type_mismatch": "ignore",
        "hole_clearance": "error",
        "hole_to_hole": "warning",
        "holes_co_located": "warning",
        "invalid_outline": "error",
        "isolated_copper": "warning",
        "item_on_disabled_layer": "error",
        "items_not_allowed": "error",
        "length_out_of_range": "error",
        "lib_footprint_issues": "warning",
        "lib_footprint_mismatch": "warning",
        "malformed_courtyard": "error",
        "microvia_drill_out_of_range": "error",
        "mirrored_text_on_front_layer": "warning",
        "missing_courtyard": "ignore",
        "missing_footprint": "warning",
        "missing_tuning_profile": "warning",
        "net_conflict": "warning",
        "nonmirrored_text_on_back_layer": "warning",
        "npth_inside_courtyard": "error",
        "padstack": "warning",
        "pth_inside_courtyard": "error",
        "shorting_items": "error",
        "silk_edge_clearance": "warning",
        "silk_over_copper": "warning",
        "silk_overlap": "warning",
        "skew_out_of_range": "error",
        "solder_mask_bridge": "error",
        "starved_thermal": "error",
        "text_height": "warning",
        "text_on_edge_cuts": "error",
        "text_thickness": "warning",
        "through_hole_pad_without_hole": "error",
        "too_many_vias": "error",
        "track_angle": "error",
        "track_dangling": "warning",
        "track_not_centered_on_via": "ignore",
        "track_on_post_machined_layer": "error",
        "track_segment_length": "error",
        "track_width": "error",
        "tracks_crossing": "error",
        "tuning_profile_track_geometries": "ignore",
        "unconnected_items": "error",
        "unresolved_variable": "error",
        "via_dangling": "warning",
        "zones_intersect": "error"
      },
      "rules": {
        "max_error": 0.005,
        "min_clearance": 0.0,
        "min_connection": 0.0,
        "min_copper_edge_clearance": 0.025,
        "min_groove_width": 0.0,
        "min_hole_clearance": 0.25,
        "min_hole_to_hole": 0.25,
        "min_microvia_diameter": 0.2,
        "min_microvia_drill": 0.1,
        "min_resolved_spokes": 2,
        "min_silk_clearance": 0.0,
        "min_text_height": 0.8,
        "min_text_thickness": 0.08,
        "min_through_hole_diameter": 0.3,
        "min_track_width": 0.2,
        "min_via_annular_width": 0.1,
        "min_via_diameter": 0.5,
        "solder_mask_to_copper_clearance": 0.0,
        "use_height_for_length_calcs": true
      },
      "teardrop_options": [
        {
          "td_onpthpad": true,
          "td_onroundshapesonly": false,
          "td_onsmdpad": true,
          "td_ontrackend": false,
          "td_onvia": true
        }
      ],
      "teardrop_parameters": [
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_round_shape",
          "td_width_to_size_filter_ratio": 0.9
        },
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_rect_shape",
          "td_width_to_size_filter_ratio": 0.9
        },
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_track_end",
          "td_width_to_size_filter_ratio": 0.9
        }
      ],
      "track_widths": [],
      "tuning_pattern_settings": {
        "diff_pair_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 1.0
        },
        "diff_pair_skew_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 0.6
        },
        "single_track_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 0.6
        }
      },
      "via_dimensions": [],
      "zones_allow_external_fillets": false
    },
    "ipc2581": {
      "bom_rev": "",
      "dist": "",
      "distpn": "",
      "internal_id": "",
      "mfg": "",
      "mpn": "",
      "sch_revision": ""
    },
    "layer_pairs": [],
    "layer_presets": [],
    "viewports": []
  },
  "boards": [],
  "component_class_settings": {
    "assignments": [],
    "meta": {
      "version": 0
    },
    "sheet_component_classes": {
      "enabled": false
    }
  },
  "cvpcb": {
    "equivalence_files": []
  },
  "libraries": {
    "pinned_footprint_libs": [],
    "pinned_symbol_libs": []
  },
  "meta": {
    "filename": "ACU7EV.kicad_pro",
    "version": 3
  },
  "net_settings": {
    "classes": [
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Default",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.127,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "CS_0",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.127,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.1143,
        "diff_pair_gap": 0.127,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.1143,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "CS_1",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.1143,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.1651,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "CS_2",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.1651,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.1143,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "CS_3",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.1143,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.1016,
        "diff_pair_gap": 0.1778,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.1016,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "CS_4",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.1016,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2032,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "CS_5",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.254,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.127,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "CS_6",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.127,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_225_SFP_CLKN",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_225_SFP_CLKP",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_485_1",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_485_2",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_505_DP_CLKN",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_505_DP_CLKP",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_505_PCIE_REFCLK",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_505_USB_CLKN",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_505_USB_CLKP",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_90OHM",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_CAN1",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_CAN2",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_DPAUX",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_CLK0",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_CLK1",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_DP0_C2M",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_DP0_M2C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_GBTCLK0_M2C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA00_CC",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA01_CC",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA02",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA03",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA04",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA05",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA06",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA07",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA08",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA09",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA10",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA11",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA12",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA13",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA14",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA15",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA16",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA17_CC",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA18_CC",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA19",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA20",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA21",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA22",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA23",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA24",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA25",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA26",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA27",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA28",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA29",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA30",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA31",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA32",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_FMC_LA33",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_GT0_DP_TX",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_GT0_DP_TX_C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_GT1_DP_TX",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_GT1_DP_TX_C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI0_RX_0",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI0_RX_1",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI0_RX_2",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI0_RX_C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_DRU_CLOCK_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_DRU_CLOCK_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_IN0_RX_0N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_IN0_RX_0P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_IN0_RX_1N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_IN0_RX_1P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_IN0_RX_2N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_IN0_RX_2P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_REC_CLOCK",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_TX0_D0N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_TX0_D0P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_TX0_D1N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_TX0_D1P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_TX0_D2N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_TX0_D2P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_TX_LVDS_OUT_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_HDMI_TX_LVDS_OUT_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_MIPI_CLK",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_MIPI_LAN0",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_MIPI_LAN1",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_CLK_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_CLK_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_REFCLK",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_RX",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX0_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX0_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX1_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX1_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX2_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX2_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX3_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX3_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX4_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX4_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX5_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX5_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX6_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX6_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX7_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX7_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PCIE_TX_C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_PHY_MDI0_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_RX_DS1",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_RX_DS2",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_RX_DS3",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_RX_DS4",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_0",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_1",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_2",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_DS1",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_DS1_C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_DS2",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_DS2_C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_DS3",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_DS3_C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_DS4",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_TX_DS4_C",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_UART_PL",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_USB",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_USB_D0",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_USB_D1",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_USB_D2",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_USB_D3",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_USB_D4",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_USB_RXN_UP",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_USB_RXP_UP",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_USB_SSTXN",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_USB_SSTXP",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_Y3",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_Y4",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_Y6",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_Y7",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "DP_Y8",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_ETH_RX",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_ETH_TX",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_HDMI_8T49N241_OUT_N",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_HDMI_8T49N241_OUT_P",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_HDMI_IN0_RX_CLKN",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_HDMI_IN0_RX_CLKP",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_IO1-DIFF",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_OTG_DATA",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_PCIE",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_PHY_MDI",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_SD_D",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "MG_SPF-DIFF",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "W10mil",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": -1,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.254,
        "tuning_profile": "",
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      }
    ],
    "meta": {
      "version": 5
    },
    "net_colors": null,
    "netclass_assignments": null,
    "netclass_patterns": [
      {
        "netclass": "W10mil",
        "pattern": "+3.3V"
      },
      {
        "netclass": "DP_225_SFP_CLKN",
        "pattern": "N24547372"
      },
      {
        "netclass": "DP_225_SFP_CLKN",
        "pattern": "225_SFP_CLKN"
      },
      {
        "netclass": "DP_225_SFP_CLKP",
        "pattern": "N24547389"
      },
      {
        "netclass": "DP_225_SFP_CLKP",
        "pattern": "225_SFP_CLKP"
      },
      {
        "netclass": "DP_485_1",
        "pattern": "485_B1"
      },
      {
        "netclass": "DP_485_1",
        "pattern": "485_A1"
      },
      {
        "netclass": "DP_485_2",
        "pattern": "485_A2"
      },
      {
        "netclass": "DP_485_2",
        "pattern": "485_B2"
      },
      {
        "netclass": "DP_505_DP_CLKN",
        "pattern": "N25916931"
      },
      {
        "netclass": "DP_505_DP_CLKN",
        "pattern": "505_DP_CLKN"
      },
      {
        "netclass": "DP_505_DP_CLKP",
        "pattern": "N25916928"
      },
      {
        "netclass": "DP_505_DP_CLKP",
        "pattern": "505_DP_CLKP"
      },
      {
        "netclass": "DP_505_PCIE_REFCLK",
        "pattern": "505_PCIE_REFCLK_N"
      },
      {
        "netclass": "DP_505_PCIE_REFCLK",
        "pattern": "505_PCIE_REFCLK_P"
      },
      {
        "netclass": "DP_505_USB_CLKN",
        "pattern": "N24545544"
      },
      {
        "netclass": "DP_505_USB_CLKN",
        "pattern": "505_USB_CLKN"
      },
      {
        "netclass": "DP_505_USB_CLKP",
        "pattern": "N24545542"
      },
      {
        "netclass": "DP_505_USB_CLKP",
        "pattern": "505_USB_CLKP"
      },
      {
        "netclass": "DP_90OHM",
        "pattern": "OTG_D_N"
      },
      {
        "netclass": "DP_90OHM",
        "pattern": "OTG_D_P"
      },
      {
        "netclass": "DP_CAN1",
        "pattern": "CAN1_CANH"
      },
      {
        "netclass": "DP_CAN1",
        "pattern": "CAN1_CANL"
      },
      {
        "netclass": "DP_CAN2",
        "pattern": "CAN2_CANL"
      },
      {
        "netclass": "DP_CAN2",
        "pattern": "CAN2_CANH"
      },
      {
        "netclass": "DP_DPAUX",
        "pattern": "DPAUX_P"
      },
      {
        "netclass": "DP_DPAUX",
        "pattern": "DPAUX_N"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY1_RXD0"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY1_RXD2"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY1_RXCTL"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY2_RXD2"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY2_RXD0"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY2_RXCTL"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY2_RXD3"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY2_RXD1"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY2_RXCK"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY1_RXD3"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY1_RXD1"
      },
      {
        "netclass": "MG_ETH_RX",
        "pattern": "PHY1_RXCK"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY1_TXD2"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY2_TXD1"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY2_TXD0"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY2_TXCTL"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY2_TXD3"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY2_TXCK"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY2_TXD2"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY1_TXCTL"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY1_TXD3"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY1_TXD1"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY1_TXD0"
      },
      {
        "netclass": "MG_ETH_TX",
        "pattern": "PHY1_TXCK"
      },
      {
        "netclass": "DP_FMC_CLK0",
        "pattern": "FMC_CLK0_P"
      },
      {
        "netclass": "DP_FMC_CLK0",
        "pattern": "FMC_CLK0_N"
      },
      {
        "netclass": "DP_FMC_CLK1",
        "pattern": "FMC_CLK1_P"
      },
      {
        "netclass": "DP_FMC_CLK1",
        "pattern": "FMC_CLK1_N"
      },
      {
        "netclass": "DP_FMC_DP0_C2M",
        "pattern": "FMC_DP0_C2M_N"
      },
      {
        "netclass": "DP_FMC_DP0_C2M",
        "pattern": "FMC_DP0_C2M_P"
      },
      {
        "netclass": "DP_FMC_DP0_M2C",
        "pattern": "FMC_DP0_M2C_P"
      },
      {
        "netclass": "DP_FMC_DP0_M2C",
        "pattern": "FMC_DP0_M2C_N"
      },
      {
        "netclass": "DP_FMC_GBTCLK0_M2C",
        "pattern": "FMC_GBTCLK0_M2C_N"
      },
      {
        "netclass": "DP_FMC_GBTCLK0_M2C",
        "pattern": "FMC_GBTCLK0_M2C_P"
      },
      {
        "netclass": "DP_FMC_LA00_CC",
        "pattern": "FMC_LA00_CC_N"
      },
      {
        "netclass": "DP_FMC_LA00_CC",
        "pattern": "FMC_LA00_CC_P"
      },
      {
        "netclass": "DP_FMC_LA01_CC",
        "pattern": "FMC_LA01_CC_N"
      },
      {
        "netclass": "DP_FMC_LA01_CC",
        "pattern": "FMC_LA01_CC_P"
      },
      {
        "netclass": "DP_FMC_LA02",
        "pattern": "FMC_LA02_N"
      },
      {
        "netclass": "DP_FMC_LA02",
        "pattern": "FMC_LA02_P"
      },
      {
        "netclass": "DP_FMC_LA03",
        "pattern": "FMC_LA03_N"
      },
      {
        "netclass": "DP_FMC_LA03",
        "pattern": "FMC_LA03_P"
      },
      {
        "netclass": "DP_FMC_LA04",
        "pattern": "FMC_LA04_N"
      },
      {
        "netclass": "DP_FMC_LA04",
        "pattern": "FMC_LA04_P"
      },
      {
        "netclass": "DP_FMC_LA05",
        "pattern": "FMC_LA05_N"
      },
      {
        "netclass": "DP_FMC_LA05",
        "pattern": "FMC_LA05_P"
      },
      {
        "netclass": "DP_FMC_LA06",
        "pattern": "FMC_LA06_P"
      },
      {
        "netclass": "DP_FMC_LA06",
        "pattern": "FMC_LA06_N"
      },
      {
        "netclass": "DP_FMC_LA07",
        "pattern": "FMC_LA07_P"
      },
      {
        "netclass": "DP_FMC_LA07",
        "pattern": "FMC_LA07_N"
      },
      {
        "netclass": "DP_FMC_LA08",
        "pattern": "FMC_LA08_N"
      },
      {
        "netclass": "DP_FMC_LA08",
        "pattern": "FMC_LA08_P"
      },
      {
        "netclass": "DP_FMC_LA09",
        "pattern": "FMC_LA09_N"
      },
      {
        "netclass": "DP_FMC_LA09",
        "pattern": "FMC_LA09_P"
      },
      {
        "netclass": "DP_FMC_LA10",
        "pattern": "FMC_LA10_P"
      },
      {
        "netclass": "DP_FMC_LA10",
        "pattern": "FMC_LA10_N"
      },
      {
        "netclass": "DP_FMC_LA11",
        "pattern": "FMC_LA11_N"
      },
      {
        "netclass": "DP_FMC_LA11",
        "pattern": "FMC_LA11_P"
      },
      {
        "netclass": "DP_FMC_LA12",
        "pattern": "FMC_LA12_N"
      },
      {
        "netclass": "DP_FMC_LA12",
        "pattern": "FMC_LA12_P"
      },
      {
        "netclass": "DP_FMC_LA13",
        "pattern": "FMC_LA13_N"
      },
      {
        "netclass": "DP_FMC_LA13",
        "pattern": "FMC_LA13_P"
      },
      {
        "netclass": "DP_FMC_LA14",
        "pattern": "FMC_LA14_P"
      },
      {
        "netclass": "DP_FMC_LA14",
        "pattern": "FMC_LA14_N"
      },
      {
        "netclass": "DP_FMC_LA15",
        "pattern": "FMC_LA15_N"
      },
      {
        "netclass": "DP_FMC_LA15",
        "pattern": "FMC_LA15_P"
      },
      {
        "netclass": "DP_FMC_LA16",
        "pattern": "FMC_LA16_N"
      },
      {
        "netclass": "DP_FMC_LA16",
        "pattern": "FMC_LA16_P"
      },
      {
        "netclass": "DP_FMC_LA17_CC",
        "pattern": "FMC_LA17_CC_P"
      },
      {
        "netclass": "DP_FMC_LA17_CC",
        "pattern": "FMC_LA17_CC_N"
      },
      {
        "netclass": "DP_FMC_LA18_CC",
        "pattern": "FMC_LA18_CC_N"
      },
      {
        "netclass": "DP_FMC_LA18_CC",
        "pattern": "FMC_LA18_CC_P"
      },
      {
        "netclass": "DP_FMC_LA19",
        "pattern": "FMC_LA19_P"
      },
      {
        "netclass": "DP_FMC_LA19",
        "pattern": "FMC_LA19_N"
      },
      {
        "netclass": "DP_FMC_LA20",
        "pattern": "FMC_LA20_N"
      },
      {
        "netclass": "DP_FMC_LA20",
        "pattern": "FMC_LA20_P"
      },
      {
        "netclass": "DP_FMC_LA21",
        "pattern": "FMC_LA21_P"
      },
      {
        "netclass": "DP_FMC_LA21",
        "pattern": "FMC_LA21_N"
      },
      {
        "netclass": "DP_FMC_LA22",
        "pattern": "FMC_LA22_P"
      },
      {
        "netclass": "DP_FMC_LA22",
        "pattern": "FMC_LA22_N"
      },
      {
        "netclass": "DP_FMC_LA23",
        "pattern": "FMC_LA23_P"
      },
      {
        "netclass": "DP_FMC_LA23",
        "pattern": "FMC_LA23_N"
      },
      {
        "netclass": "DP_FMC_LA24",
        "pattern": "FMC_LA24_P"
      },
      {
        "netclass": "DP_FMC_LA24",
        "pattern": "FMC_LA24_N"
      },
      {
        "netclass": "DP_FMC_LA25",
        "pattern": "FMC_LA25_N"
      },
      {
        "netclass": "DP_FMC_LA25",
        "pattern": "FMC_LA25_P"
      },
      {
        "netclass": "DP_FMC_LA26",
        "pattern": "FMC_LA26_N"
      },
      {
        "netclass": "DP_FMC_LA26",
        "pattern": "FMC_LA26_P"
      },
      {
        "netclass": "DP_FMC_LA27",
        "pattern": "FMC_LA27_N"
      },
      {
        "netclass": "DP_FMC_LA27",
        "pattern": "FMC_LA27_P"
      },
      {
        "netclass": "DP_FMC_LA28",
        "pattern": "FMC_LA28_N"
      },
      {
        "netclass": "DP_FMC_LA28",
        "pattern": "FMC_LA28_P"
      },
      {
        "netclass": "DP_FMC_LA29",
        "pattern": "FMC_LA29_P"
      },
      {
        "netclass": "DP_FMC_LA29",
        "pattern": "FMC_LA29_N"
      },
      {
        "netclass": "DP_FMC_LA30",
        "pattern": "FMC_LA30_N"
      },
      {
        "netclass": "DP_FMC_LA30",
        "pattern": "FMC_LA30_P"
      },
      {
        "netclass": "DP_FMC_LA31",
        "pattern": "FMC_LA31_P"
      },
      {
        "netclass": "DP_FMC_LA31",
        "pattern": "FMC_LA31_N"
      },
      {
        "netclass": "DP_FMC_LA32",
        "pattern": "FMC_LA32_N"
      },
      {
        "netclass": "DP_FMC_LA32",
        "pattern": "FMC_LA32_P"
      },
      {
        "netclass": "DP_FMC_LA33",
        "pattern": "FMC_LA33_N"
      },
      {
        "netclass": "DP_FMC_LA33",
        "pattern": "FMC_LA33_P"
      },
      {
        "netclass": "DP_GT0_DP_TX",
        "pattern": "GT0_DP_TX_P"
      },
      {
        "netclass": "DP_GT0_DP_TX",
        "pattern": "GT0_DP_TX_N"
      },
      {
        "netclass": "DP_GT0_DP_TX_C",
        "pattern": "GT0_DP_TX_C_N"
      },
      {
        "netclass": "DP_GT0_DP_TX_C",
        "pattern": "GT0_DP_TX_C_P"
      },
      {
        "netclass": "DP_GT1_DP_TX",
        "pattern": "GT1_DP_TX_P"
      },
      {
        "netclass": "DP_GT1_DP_TX",
        "pattern": "GT1_DP_TX_N"
      },
      {
        "netclass": "DP_GT1_DP_TX_C",
        "pattern": "GT1_DP_TX_C_N"
      },
      {
        "netclass": "DP_GT1_DP_TX_C",
        "pattern": "GT1_DP_TX_C_P"
      },
      {
        "netclass": "DP_HDMI0_RX_0",
        "pattern": "HDMI0_RX_0N"
      },
      {
        "netclass": "DP_HDMI0_RX_0",
        "pattern": "HDMI0_RX_0P"
      },
      {
        "netclass": "DP_HDMI0_RX_1",
        "pattern": "HDMI0_RX_1P"
      },
      {
        "netclass": "DP_HDMI0_RX_1",
        "pattern": "HDMI0_RX_1N"
      },
      {
        "netclass": "DP_HDMI0_RX_2",
        "pattern": "HDMI0_RX_2N"
      },
      {
        "netclass": "DP_HDMI0_RX_2",
        "pattern": "HDMI0_RX_2P"
      },
      {
        "netclass": "DP_HDMI0_RX_C",
        "pattern": "HDMI0_RX_CN"
      },
      {
        "netclass": "DP_HDMI0_RX_C",
        "pattern": "HDMI0_RX_CP"
      },
      {
        "netclass": "MG_HDMI_8T49N241_OUT_N",
        "pattern": "HDMI_8T49N241_OUT_N"
      },
      {
        "netclass": "MG_HDMI_8T49N241_OUT_N",
        "pattern": "N25641497"
      },
      {
        "netclass": "MG_HDMI_8T49N241_OUT_N",
        "pattern": "N25344461"
      },
      {
        "netclass": "MG_HDMI_8T49N241_OUT_P",
        "pattern": "HDMI_8T49N241_OUT_P"
      },
      {
        "netclass": "MG_HDMI_8T49N241_OUT_P",
        "pattern": "N25641494"
      },
      {
        "netclass": "MG_HDMI_8T49N241_OUT_P",
        "pattern": "N25344453"
      },
      {
        "netclass": "DP_HDMI_DRU_CLOCK_N",
        "pattern": "N25296078"
      },
      {
        "netclass": "DP_HDMI_DRU_CLOCK_N",
        "pattern": "HDMI_DRU_CLOCK_N"
      },
      {
        "netclass": "DP_HDMI_DRU_CLOCK_P",
        "pattern": "HDMI_DRU_CLOCK_P"
      },
      {
        "netclass": "DP_HDMI_DRU_CLOCK_P",
        "pattern": "N25296083"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_0N",
        "pattern": "N25309248"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_0N",
        "pattern": "HDMI_IN0_RX_0N"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_0P",
        "pattern": "N25309240"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_0P",
        "pattern": "HDMI_IN0_RX_0P"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_1N",
        "pattern": "N25309242"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_1N",
        "pattern": "HDMI_IN0_RX_1N"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_1P",
        "pattern": "N25309234"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_1P",
        "pattern": "HDMI_IN0_RX_1P"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_2N",
        "pattern": "N25309236"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_2N",
        "pattern": "HDMI_IN0_RX_2N"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_2P",
        "pattern": "N25309238"
      },
      {
        "netclass": "DP_HDMI_IN0_RX_2P",
        "pattern": "HDMI_IN0_RX_2P"
      },
      {
        "netclass": "MG_HDMI_IN0_RX_CLKN",
        "pattern": "HDMI_IN0_RX_CLKN"
      },
      {
        "netclass": "MG_HDMI_IN0_RX_CLKP",
        "pattern": "HDMI_IN0_RX_CLKP"
      },
      {
        "netclass": "DP_HDMI_REC_CLOCK",
        "pattern": "HDMI_REC_CLOCK_N"
      },
      {
        "netclass": "DP_HDMI_REC_CLOCK",
        "pattern": "HDMI_REC_CLOCK_P"
      },
      {
        "netclass": "DP_HDMI_TX0_D0N",
        "pattern": "HDMI_TX0_D0N"
      },
      {
        "netclass": "DP_HDMI_TX0_D0N",
        "pattern": "N25297089"
      },
      {
        "netclass": "DP_HDMI_TX0_D0P",
        "pattern": "N25297084"
      },
      {
        "netclass": "DP_HDMI_TX0_D0P",
        "pattern": "HDMI_TX0_D0P"
      },
      {
        "netclass": "DP_HDMI_TX0_D1N",
        "pattern": "HDMI_TX0_D1N"
      },
      {
        "netclass": "DP_HDMI_TX0_D1N",
        "pattern": "N25297081"
      },
      {
        "netclass": "DP_HDMI_TX0_D1P",
        "pattern": "HDMI_TX0_D1P"
      },
      {
        "netclass": "DP_HDMI_TX0_D1P",
        "pattern": "N25297080"
      },
      {
        "netclass": "DP_HDMI_TX0_D2N",
        "pattern": "N25297061"
      },
      {
        "netclass": "DP_HDMI_TX0_D2N",
        "pattern": "HDMI_TX0_D2N"
      },
      {
        "netclass": "DP_HDMI_TX0_D2P",
        "pattern": "N25297074"
      },
      {
        "netclass": "DP_HDMI_TX0_D2P",
        "pattern": "HDMI_TX0_D2P"
      },
      {
        "netclass": "DP_HDMI_TX_LVDS_OUT_N",
        "pattern": "HDMI_TX_LVDS_OUT_N"
      },
      {
        "netclass": "DP_HDMI_TX_LVDS_OUT_N",
        "pattern": "N25297095"
      },
      {
        "netclass": "DP_HDMI_TX_LVDS_OUT_P",
        "pattern": "HDMI_TX_LVDS_OUT_P"
      },
      {
        "netclass": "DP_HDMI_TX_LVDS_OUT_P",
        "pattern": "N25297094"
      },
      {
        "netclass": "MG_IO1-DIFF",
        "pattern": "FAN_PWM"
      },
      {
        "netclass": "DP_MIPI_CLK",
        "pattern": "MIPI_CLK_N"
      },
      {
        "netclass": "DP_MIPI_CLK",
        "pattern": "MIPI_CLK_P"
      },
      {
        "netclass": "DP_MIPI_LAN0",
        "pattern": "MIPI_LAN0_N"
      },
      {
        "netclass": "DP_MIPI_LAN0",
        "pattern": "MIPI_LAN0_P"
      },
      {
        "netclass": "DP_MIPI_LAN1",
        "pattern": "MIPI_LAN1_N"
      },
      {
        "netclass": "DP_MIPI_LAN1",
        "pattern": "MIPI_LAN1_P"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_STP"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_DATA6"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_NXT"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_DATA2"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_DATA0"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_DATA1"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_DATA3"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_CLK"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_DATA7"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_DIR"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_DATA5"
      },
      {
        "netclass": "MG_OTG_DATA",
        "pattern": "USB_DATA4"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX7_N"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX7_P"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX6_N"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX6_P"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX5_N"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX5_P"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX4_P"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX4_N"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX0_N"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX1_N"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX0_P"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX2_N"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX3_P"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX2_P"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX3_N"
      },
      {
        "netclass": "MG_PCIE",
        "pattern": "PCIE_RX1_P"
      },
      {
        "netclass": "DP_PCIE_CLK_N",
        "pattern": "N25208409"
      },
      {
        "netclass": "DP_PCIE_CLK_N",
        "pattern": "PCIE_CLK_N"
      },
      {
        "netclass": "DP_PCIE_CLK_P",
        "pattern": "N25208411"
      },
      {
        "netclass": "DP_PCIE_CLK_P",
        "pattern": "PCIE_CLK_P"
      },
      {
        "netclass": "DP_PCIE_REFCLK",
        "pattern": "PCIE_REFCLK_P"
      },
      {
        "netclass": "DP_PCIE_REFCLK",
        "pattern": "PCIE_REFCLK_N"
      },
      {
        "netclass": "DP_PCIE_RX",
        "pattern": "PCIE_RX_P"
      },
      {
        "netclass": "DP_PCIE_RX",
        "pattern": "PCIE_RX_N"
      },
      {
        "netclass": "DP_PCIE_TX",
        "pattern": "PCIE_TX_N"
      },
      {
        "netclass": "DP_PCIE_TX",
        "pattern": "PCIE_TX_P"
      },
      {
        "netclass": "DP_PCIE_TX0_N",
        "pattern": "N25208362"
      },
      {
        "netclass": "DP_PCIE_TX0_N",
        "pattern": "PCIE_TX0_N"
      },
      {
        "netclass": "DP_PCIE_TX0_P",
        "pattern": "N25208364"
      },
      {
        "netclass": "DP_PCIE_TX0_P",
        "pattern": "PCIE_TX0_P"
      },
      {
        "netclass": "DP_PCIE_TX1_N",
        "pattern": "N25208366"
      },
      {
        "netclass": "DP_PCIE_TX1_N",
        "pattern": "PCIE_TX1_N"
      },
      {
        "netclass": "DP_PCIE_TX1_P",
        "pattern": "N25208368"
      },
      {
        "netclass": "DP_PCIE_TX1_P",
        "pattern": "PCIE_TX1_P"
      },
      {
        "netclass": "DP_PCIE_TX2_N",
        "pattern": "N25208370"
      },
      {
        "netclass": "DP_PCIE_TX2_N",
        "pattern": "PCIE_TX2_N"
      },
      {
        "netclass": "DP_PCIE_TX2_P",
        "pattern": "N25208372"
      },
      {
        "netclass": "DP_PCIE_TX2_P",
        "pattern": "PCIE_TX2_P"
      },
      {
        "netclass": "DP_PCIE_TX3_N",
        "pattern": "N25208374"
      },
      {
        "netclass": "DP_PCIE_TX3_N",
        "pattern": "PCIE_TX3_N"
      },
      {
        "netclass": "DP_PCIE_TX3_P",
        "pattern": "N25208376"
      },
      {
        "netclass": "DP_PCIE_TX3_P",
        "pattern": "PCIE_TX3_P"
      },
      {
        "netclass": "DP_PCIE_TX4_N",
        "pattern": "N25208593"
      },
      {
        "netclass": "DP_PCIE_TX4_N",
        "pattern": "PCIE_TX4_N"
      },
      {
        "netclass": "DP_PCIE_TX4_P",
        "pattern": "N25208595"
      },
      {
        "netclass": "DP_PCIE_TX4_P",
        "pattern": "PCIE_TX4_P"
      },
      {
        "netclass": "DP_PCIE_TX5_N",
        "pattern": "N25208619"
      },
      {
        "netclass": "DP_PCIE_TX5_N",
        "pattern": "PCIE_TX5_N"
      },
      {
        "netclass": "DP_PCIE_TX5_P",
        "pattern": "N25208637"
      },
      {
        "netclass": "DP_PCIE_TX5_P",
        "pattern": "PCIE_TX5_P"
      },
      {
        "netclass": "DP_PCIE_TX6_N",
        "pattern": "N25208653"
      },
      {
        "netclass": "DP_PCIE_TX6_N",
        "pattern": "PCIE_TX6_N"
      },
      {
        "netclass": "DP_PCIE_TX6_P",
        "pattern": "N25208655"
      },
      {
        "netclass": "DP_PCIE_TX6_P",
        "pattern": "PCIE_TX6_P"
      },
      {
        "netclass": "DP_PCIE_TX7_N",
        "pattern": "N25208669"
      },
      {
        "netclass": "DP_PCIE_TX7_N",
        "pattern": "PCIE_TX7_N"
      },
      {
        "netclass": "DP_PCIE_TX7_P",
        "pattern": "N25208689"
      },
      {
        "netclass": "DP_PCIE_TX7_P",
        "pattern": "PCIE_TX7_P"
      },
      {
        "netclass": "DP_PCIE_TX_C",
        "pattern": "PCIE_TX_C_P"
      },
      {
        "netclass": "DP_PCIE_TX_C",
        "pattern": "PCIE_TX_C_N"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY2_MDI3_N"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY2_MDI1_N"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY2_MDI1_P"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY2_MDI3_P"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY2_MDI2_P"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY2_MDI0_P"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY2_MDI2_N"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY2_MDI0_N"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY1_MDI3_P"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY1_MDI1_P"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY1_MDI1_N"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY1_MDI3_N"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY1_MDI2_P"
      },
      {
        "netclass": "MG_PHY_MDI",
        "pattern": "PHY1_MDI2_N"
      },
      {
        "netclass": "DP_PHY_MDI0_N",
        "pattern": "PHY1_MDI0_P"
      },
      {
        "netclass": "DP_PHY_MDI0_N",
        "pattern": "PHY1_MDI0_N"
      },
      {
        "netclass": "DP_RX_DS1",
        "pattern": "RX_DS1_N"
      },
      {
        "netclass": "DP_RX_DS1",
        "pattern": "RX_DS1_P"
      },
      {
        "netclass": "DP_RX_DS2",
        "pattern": "RX_DS2_N"
      },
      {
        "netclass": "DP_RX_DS2",
        "pattern": "RX_DS2_P"
      },
      {
        "netclass": "DP_RX_DS3",
        "pattern": "RX_DS3_N"
      },
      {
        "netclass": "DP_RX_DS3",
        "pattern": "RX_DS3_P"
      },
      {
        "netclass": "DP_RX_DS4",
        "pattern": "RX_DS4_N"
      },
      {
        "netclass": "DP_RX_DS4",
        "pattern": "RX_DS4_P"
      },
      {
        "netclass": "MG_SD_D",
        "pattern": "SD_CLK"
      },
      {
        "netclass": "MG_SD_D",
        "pattern": "SD_CMD"
      },
      {
        "netclass": "MG_SD_D",
        "pattern": "SD_D0"
      },
      {
        "netclass": "MG_SD_D",
        "pattern": "SD_D2"
      },
      {
        "netclass": "MG_SD_D",
        "pattern": "SD_D1"
      },
      {
        "netclass": "MG_SD_D",
        "pattern": "SD_D3"
      },
      {
        "netclass": "MG_SPF-DIFF",
        "pattern": "SFP2_RX_N"
      },
      {
        "netclass": "MG_SPF-DIFF",
        "pattern": "SFP2_TX_N"
      },
      {
        "netclass": "MG_SPF-DIFF",
        "pattern": "SFP1_TX_N"
      },
      {
        "netclass": "MG_SPF-DIFF",
        "pattern": "SFP2_TX_P"
      },
      {
        "netclass": "MG_SPF-DIFF",
        "pattern": "SFP1_RX_P"
      },
      {
        "netclass": "MG_SPF-DIFF",
        "pattern": "SFP1_TX_P"
      },
      {
        "netclass": "MG_SPF-DIFF",
        "pattern": "SFP2_RX_P"
      },
      {
        "netclass": "MG_SPF-DIFF",
        "pattern": "SFP1_RX_N"
      },
      {
        "netclass": "DP_TX_0",
        "pattern": "TX_0P"
      },
      {
        "netclass": "DP_TX_0",
        "pattern": "TX_0N"
      },
      {
        "netclass": "DP_TX_1",
        "pattern": "TX_1P"
      },
      {
        "netclass": "DP_TX_1",
        "pattern": "TX_1N"
      },
      {
        "netclass": "DP_TX_2",
        "pattern": "TX_2P"
      },
      {
        "netclass": "DP_TX_2",
        "pattern": "TX_2N"
      },
      {
        "netclass": "DP_TX_C",
        "pattern": "TX_CP"
      },
      {
        "netclass": "DP_TX_C",
        "pattern": "TX_CN"
      },
      {
        "netclass": "DP_TX_DS1",
        "pattern": "TX_DS1_N"
      },
      {
        "netclass": "DP_TX_DS1",
        "pattern": "TX_DS1_P"
      },
      {
        "netclass": "DP_TX_DS1_C",
        "pattern": "TX_DS1_C_P"
      },
      {
        "netclass": "DP_TX_DS1_C",
        "pattern": "TX_DS1_C_N"
      },
      {
        "netclass": "DP_TX_DS2",
        "pattern": "TX_DS2_N"
      },
      {
        "netclass": "DP_TX_DS2",
        "pattern": "TX_DS2_P"
      },
      {
        "netclass": "DP_TX_DS2_C",
        "pattern": "TX_DS2_C_N"
      },
      {
        "netclass": "DP_TX_DS2_C",
        "pattern": "TX_DS2_C_P"
      },
      {
        "netclass": "DP_TX_DS3",
        "pattern": "TX_DS3_N"
      },
      {
        "netclass": "DP_TX_DS3",
        "pattern": "TX_DS3_P"
      },
      {
        "netclass": "DP_TX_DS3_C",
        "pattern": "TX_DS3_C_N"
      },
      {
        "netclass": "DP_TX_DS3_C",
        "pattern": "TX_DS3_C_P"
      },
      {
        "netclass": "DP_TX_DS4",
        "pattern": "TX_DS4_N"
      },
      {
        "netclass": "DP_TX_DS4",
        "pattern": "TX_DS4_P"
      },
      {
        "netclass": "DP_TX_DS4_C",
        "pattern": "TX_DS4_C_N"
      },
      {
        "netclass": "DP_TX_DS4_C",
        "pattern": "TX_DS4_C_P"
      },
      {
        "netclass": "DP_UART_PL",
        "pattern": "N23663238"
      },
      {
        "netclass": "DP_UART_PL",
        "pattern": "N23663240"
      },
      {
        "netclass": "DP_USB",
        "pattern": "N16524061"
      },
      {
        "netclass": "DP_USB",
        "pattern": "N16523963"
      },
      {
        "netclass": "DP_USB_D0",
        "pattern": "USB_DP0"
      },
      {
        "netclass": "DP_USB_D0",
        "pattern": "USB_DM0"
      },
      {
        "netclass": "DP_USB_D1",
        "pattern": "USB_DM1"
      },
      {
        "netclass": "DP_USB_D1",
        "pattern": "USB_DP1"
      },
      {
        "netclass": "DP_USB_D2",
        "pattern": "USB_DM2"
      },
      {
        "netclass": "DP_USB_D2",
        "pattern": "USB_DP2"
      },
      {
        "netclass": "DP_USB_D3",
        "pattern": "USB_DM3"
      },
      {
        "netclass": "DP_USB_D3",
        "pattern": "USB_DP3"
      },
      {
        "netclass": "DP_USB_D4",
        "pattern": "USB_DM4"
      },
      {
        "netclass": "DP_USB_D4",
        "pattern": "USB_DP4"
      },
      {
        "netclass": "DP_USB_RXN_UP",
        "pattern": "USB_RXN_UP"
      },
      {
        "netclass": "DP_USB_RXN_UP",
        "pattern": "USB_SSRXN"
      },
      {
        "netclass": "DP_USB_RXP_UP",
        "pattern": "USB_RXP_UP"
      },
      {
        "netclass": "DP_USB_RXP_UP",
        "pattern": "USB_SSRXP"
      },
      {
        "netclass": "DP_USB_SSTXN",
        "pattern": "USB_TXN_UP"
      },
      {
        "netclass": "DP_USB_SSTXN",
        "pattern": "USB_SSTXN"
      },
      {
        "netclass": "DP_USB_SSTXP",
        "pattern": "USB_TXP_UP"
      },
      {
        "netclass": "DP_USB_SSTXP",
        "pattern": "USB_SSTXP"
      },
      {
        "netclass": "DP_Y3",
        "pattern": "N25043434"
      },
      {
        "netclass": "DP_Y3",
        "pattern": "N25043442"
      },
      {
        "netclass": "DP_Y4",
        "pattern": "N25044098"
      },
      {
        "netclass": "DP_Y4",
        "pattern": "N25044106"
      },
      {
        "netclass": "DP_Y6",
        "pattern": "N24545918"
      },
      {
        "netclass": "DP_Y6",
        "pattern": "N24545912"
      },
      {
        "netclass": "DP_Y7",
        "pattern": "N25342533"
      },
      {
        "netclass": "DP_Y7",
        "pattern": "N25342525"
      },
      {
        "netclass": "DP_Y8",
        "pattern": "N25639886"
      },
      {
        "netclass": "DP_Y8",
        "pattern": "N25639880"
      }
    ]
  },
  "pcbnew": {
    "last_paths": {
      "idf": "",
      "netlist": "",
      "plot": "",
      "specctra_dsn": "",
      "vrml": ""
    },
    "page_layout_descr_file": ""
  },
  "schematic": {
    "bus_aliases": {},
    "legacy_lib_dir": "",
    "legacy_lib_list": [],
    "top_level_sheets": []
  },
  "sheets": [],
  "text_variables": {},
  "tuning_profiles": {
    "meta": {
      "version": 0
    },
    "tuning_profiles_impedance_geometric": []
  }
}
